Open topic with navigation

# Video Server Analysis Task Parameters

The parameters in this section customize the `VideoServerAnalysis` task.

This task runs analysis on videos that are associated with documents and have the field `AUTN_NEEDS_VIDEO_SERVER_ANALYSIS`. You must add this field to the documents that you want to analyze. You can add the field using a Lua script.

You can run the `VideoServerAnalysis` task as a Pre or Post task. When you configure the task, use the `Pre` or `Post` parameter to specify the name of a section in the CFS configuration file that contains the task settings:

    [ImportTasks]
    Post0=Lua:DetectVideos.lua
    Post1=VideoServerAnalysis:VideoServerSettings

    [VideoServerSettings]
    VideoServerHost=server:14000,server2:14000
    VideoServerConfigurationName=broadcast
    VideoAnalysisTransform=xslt/VideoServerAnalysisTransform.xsl

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm