Open topic with navigation

# ImageServerPort

The ACI port of the Image Server.

Note: If you want to use more than one Image Server for analyzing images, do not set this parameter. Set the ACI port for each Image Server in the ImageServerHost parameter.

Type: | Integer
Default: |
Required | No
Configuration Section: | Any section that you have defined for Image Server settings
Example: | `ImageServerHost=ImageServer ImageServerPort=18000`
See Also: | ImageServerHost

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm