Open topic with navigation

# ImageAnalysisPollMilliseconds

The amount of time that CFS waits before polling Image Server to see if an asynchronous request has completed, in milliseconds.

Type: | Integer
Default: | 5000
Required | No
Configuration Section: | Any section that you have defined for an `ImageServerAnalysis` task
Example: | `ImageAnalysisPollMilliseconds=3000`
See Also: | ImageAnalysisSynchronous

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm