Open topic with navigation

# PerfMonCounterMinN

The minimum value permitted for a performance counter. If the performance counter falls below this value, the connector pauses.

Note: Performance monitoring is supported on Windows platforms only.

Type: | Integer
Default: | ``
Required: | No
Configuration Section: | TaskName or FetchTasks
Example: | `PerfMonCounterName1=\\hostname\Memory\Available MBytes PerfMonCounterMin1=1024`
See Also: | PerfMonAvgOverReadings PerfMonCounterMaxN PerfMonCounterNameN PerfMonQueryFrequency

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm