Open topic with navigation

# NavLinksToFollow

A bit-wise mask number specifying the types of link the connector follows. You can create the number by adding together the following values as required:

1 | Follow `frame` links.
2 | Follow `href` links.
4 | Follow `location.href` links.
8 | Follow `http-equiv` links.
16 | Follow standard link definitions, such as anchor tags and the custom links defined by `NavLinkDefStartCSVs` and `NavLinkDefEndCSVs`.
128 | Follow links that are in comments.

To follow all links use the default value.

Type: | Long
Default: | 268435455
Required: | No
Configuration Section: | TaskName or Default
Example: | `NavLinksToFollow=10`
See Also: | NavLinkDefStartCSVs NavLinkDefEndCSVs NavLinkDefPostfixCSVs NavLinkDefPrefixCSVs

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm