Open topic with navigation

# Configure Incoming SSL Connections

To configure a connector or Connector Framework Server to accept data sent to its ACI port over SSL, follow these steps.

To configure an incoming SSL Connection

1. Stop the connector or CFS.
2. Open the configuration file in a text editor.
3. In the `[Server]` section set the `SSLConfig` parameter to specify the name of a section in the configuration file for the SSL settings. For example:

       [Server]
       SSLConfig=SSLOptions

4. Create a new section in the configuration file (the name must match the name you used in the `SSLConfig` parameter). Then, use the SSL configuration parameters to specify the details for the connection. You must set the following parameters:

   `SSLMethod` | The SSL protocol to use.
   `SSLCertificate` | The SSL certificate to use (in PEM format).
   `SSLPrivateKey` | The private key for the SSL certificate (in PEM format).

   For example:

       [SSLOptions]
       SSLMethod=SSLV23
       SSLCertificate=host1.crt
       SSLPrivateKey=host1.key

5. Save and close the configuration file.
6. Restart the connector or CFS.

Related Topics

- Start and Stop the Connector

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm