Open topic with navigation

# SleepBetweenRequests

The length of time (in milliseconds) that the IDOL Community Component mailing operation must wait after it has responded to a request before it can respond to the next request. You can use this option to slow the mailing operation down if it takes too much processing time away from IDOL Community Component.

Type: | Long
Default: | 0
Allowed Range: | Minimum: 0 Maximum: 1638400
Required: | No
Configuration Section: | `MyCustomFunctionality`
Example: | `SleepBetweenRequests=60`
See Also: | RunMailer

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm