Open topic with navigation

# TCPReceiveWindowSize

The TCP receive window size to use when the service receives data. This parameter sets the size of the socket receiving buffers for all IDOL components.

Use this parameter to tune network performance based on bandwidth and client to server round-trip times. Generally, a higher value improves performance in a high-bandwidth, high-delay network, and a lower value improves performance in a low-bandwidth, low-delay network.

Type: | Long
Default: | 6193
Allowed Range: | Minimum: 1024 Maximum: 1048576
Required: | No
Configuration Section: | Service
Example: | `TCPReceiveWindowSize=65536`
See Also: |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm