Open topic with navigation

# ControlTimeout

The number of seconds after which to time out requests to stop, start, or restart services, if there is no response.

Type: | Long
Default: | 40
Required: | No
Configuration Section: | Server
Example: | `ControlTimeout=60`
See Also: |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm