Open topic with navigation

# ThreadStatus

Displays a list of all ACI threads and specifies what each thread is doing.

## Example

    http://12.3.4.56:9000/action=ThreadStatus

This action uses port `9000` to request thread information from a component, which is located on a machine with the IP address `12.3.4.56`.

## Parameters

Parameter | Description | Required
--- | --- | ---
ActionID | A string to use to identify an ACI action. |
EncryptResponse | Encrypt the output. |
FileName | The file to write output to. |
ForceTemplateRefresh | Forces the server to load the template from disk. |
Output | Write output to a file. |
ResponseFormat | The format of the action output. |
Template | The template to use for the action output. |
TemplateParamCSVs | A list of variables to use for the specified template. |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm