Open topic with navigation

# Index Proxy Configuration Parameters

This section describes the configuration parameters that you can set to enable the proxying of index commands through the index port using the GET or POST methods.

For example:

    [IndexProxy]
    IndexPort=40201
    IndexClients=*

Controller checks the `[IndexProxy]` section first; if this section does contain the required parameters, it checks the `[Server]` section.

ChunkSize
IndexClients
IndexPort
Port
SSLConfig
Threads
Timeout

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm