Open topic with navigation

# ShutDownEnginePeriods

A comma-separated list of values of time periods that correspond to child servers that are powered down when a roll over occurs. The values are days relative to today.

Note: A zero value corresponds to a child server indexing data during the current period, a positive value corresponds to a child server that index data in the future, and a negative value corresponds to a child server that indexed data in the past.

Type: | String
Default: |
Required: | No
Configuration Section: | DAHServer `N`
Example: | `ShutDownEnginePeriods=0,-1` Shuts down the child server that is about to index data today and the child server that indexed data yesterday.
See Also: | StartUpEnginePeriods

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm