Open topic with navigation

# ServiceStatusClients

The IP addresses or names of clients that can request status information from a service. These clients cannot control the service. Separate multiple individual addresses with commas. There must be no space before or after the comma.

You can use wildcards in the IP addresses. For example, type `187.*.*.*` to permit any machine whose IP address begins with `187` to access the service's status. You can also filter the `ServiceStatusClients` parameter using CIDR notation.

Type: | String
Default: | None
Required: | Yes
Configuration Section: | Service
Example: | `ServiceStatusClients=localhost,127.0.0.1`
See Also: | ServiceACIMode ServiceControlClients ServiceHost ServicePort

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm