Open topic with navigation

# Port

The ACI port of the `N`-th DAH.

Type: | Integer
Default: | 17000
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1025 Maximum: 65535
Required: | Yes
Configuration Section: | DAHServer `N`
Example: | `Port=9000`
See Also: | Host

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm