Open topic with navigation

# IDOLServer`N` Configuration

In the `[DistributionIDOLServers]` section you must create a `[IDOLServerN]` subsection for each IDOL server that the Distributed Index Handler communicates with. Each `[IDOLServerN]` subsection specifies the host and ACI port of a child IDOL server. Note that you must number child IDOL server sections in consecutive order, starting from 0.

For example:

    [DistributionIDOLServers]
    Number=2

    [IDOLServer0]
    Host=localhost
    Port=9000

    [IDOLServer1]
    Host=1.23.45.6
    Port=9000
    UpdateOnly=true

DistributeByFieldsValues

Host

Polling

Port

UpdateOnly

ServiceSSLConfig

SSLConfig

Weight

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm