Open topic with navigation

# KeyAtLeastSec

The maximum time interval in seconds between keyframes. If the engine has not detected a scene change after this interval, the frame at the end of the interval is selected as a keyframe.

Type: | Integer
Default: | Unlimited
Required: | No
Configuration Section: | TaskName
Example: | `KeyAtLeastSec=10`
See Also: | KeyAtMostSec

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm