Open topic with navigation

# Image Encoder Engine Configuration Parameters

The ImageEncoder engine saves image records to disk as image files.

To configure an encoder task that uses the Image Encoder engine, you can set the following parameters:

Configuration Parameter | Description
--- | ---
Crop | Specifies whether images are cropped to show only the region identified by an analysis engine.
CropBorder | The size of the border to add around any output image that has been cropped.
CropBorderUnit | The units to use for specifying the size of the border around any output image that has been cropped.
Format | The image format for the output files.
FrameRateMax | The maximum number of images to save per second of video.
ImageInput | The names of the image tracks that you want to encode.
ImageSize | The output image size in pixels.
InputQueueSize | The maximum number of records to queue for encoding, for each input.
OutputPath | The path and file name for the output files.
Type | The type of encoding engine to use. Set this parameter to `imageencoder`.
URLBase | The base URL that is used to access the image.

The Image Encoder produces a proxy track, named `taskName.Proxy`, where `taskName` is the name of the encoding task.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm