Open topic with navigation

# MinRead

The minimum number of consecutive frames in which a plate must be visible before a result is returned, if the Integration parameter is set to `moving`.

Type: | Integer
Default: | 3
Required: | No
Configuration Section: | TaskName
Example: | `MinRead=5`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm