Open topic with navigation

# RejectReadsWithInvalidGaps

Specifies whether to reject number plate reads with gaps in the wrong place. For example, in the UK the number plate AB12 DEF would be permitted by the number plate formats but AB 12DEF would be considered invalid.

Type: | Boolean
Default: | True
Required: | No
Configuration Section: | TaskName
Example: | `RejectReadsWithInvalidGaps=False`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm