Open topic with navigation

# GUID

The Milestone GUID of the camera that the events should be associated with (the GUID of the camera that supplied the video). For information about finding the camera GUID, refer to the Milestone documentation.

You do not have to specify the camera GUID if you are ingesting video using the Milestone ingest engine. If you do not specify a GUID, Media Server automatically associates alarms to the camera that the Milestone ingest engine received the video from.

Type: | String
Default: |
Required: | Yes, unless you are ingesting video from Milestone using the Milestone ingest engine
Configuration Section: | TaskName
Example: |
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm