Open topic with navigation

# OutputInterval

The amount of video content represented by each output document, in seconds.

For example, if you set `OutputInterval=30` and `IntervalsPerAsset=10`, Media Server sends documents to Broadcast Monitoring that represent 30 seconds of video content. After 10 of these documents have been sent to Broadcast Monitoring and the asset represents 5 minutes of video, Media Server starts a new asset.

You could set `OutputInterval=300` and `IntervalsPerAsset=1` to achieve the same result, but this would delay the indexing of data until Media Server had processed 5 minutes of video content.

Type: | Integer
Default: |
Required: | No
Configuration Section: | TaskName
Example: | `OutputInterval=30`
See Also: | IntervalsPerAsset

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm