Open topic with navigation

# Region

Specifies a region of an image to process, instead of processing the whole image.

Specify the region using a comma-separated list of values in the order: `left`,`top`,`width`,`height`.

where,

`left` | is the distance from the left edge of the image to the left edge of the region.
`top` | is the distance from the top edge of the image to the top edge of the region.
`width` | is the width of the region.
`height` | is the height of the region.

Depending on the setting of the RegionUnit parameter, values are given in either pixels or as percentages of the image dimensions.

Type: | Comma-separated list of integers
Default: | None
Required: | No
Configuration Section: | TaskName
Example: | `Region=50,50,200,100`
See Also: | RegionUnit

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm