Open topic with navigation

# MaxConsecutiveTries

The maximum number of attempts that Media Server makes to connect to the servers listed in the SpeakerIDServers parameter.

Media Server initially attempts to connect to the first server in the list. If the connection fails, Media Server tries to connect to the next server in the list, and so on. On reaching the end of the servers list without achieving a connection, Media Server pauses for 10 seconds before attempting to connect to the first server in the list again. Media Server continues attempting to connect to the servers until it reaches the maximum number of attempts specified in the `MaxConsecutiveTries` parameter. Media Server then stops processing the session. If `MaxConsecutiveTries` is set to `0`, Media Server continues attempting to connect to the IDOL Speech Servers indefinitely.

During live ingest, HPE recommends setting `MaxConsecutiveTries` to `0` so that the session is not stopped. When ingesting files, you might want the session to fail immediately so that another component can try to process the file on a different Media Server and IDOL Speech Server setup.

Type: | Integer
Default: | 0
Required: | No
Configuration Section: | TaskName
Example: | `MaxConsecutiveTries=2`
See Also: | ErrorMessage

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm