Open topic with navigation

# Example Results

The `GetResults` action displays the audio preprocessing results as XML in your Web browser. You can also open the .ctm file from the configured IDOL Speech Server temporary directory (or another location if you specified a path in the `Out` parameter).

## Audio Categorization Mode

The following is an example of results produced by the audio categorization mode.

`1` | `A` | `22.800` | `1.120` | `Music/Noise` | `0.000`
`1` | `A` | `23.920` | `0.500` | `Speech` | `0.000`
`1` | `A` | `24.420` | `0.580` | `Silence` | `0.000`
`1` | `A` | `25.000` | `2.280` | `Speech` | `0.000`
`1` | `A` | `27.280` | `1.570` | `Speech` | `0.000`
`1` | `A` | `28.850` | `0.500` | `Silence` | `0.000`
`1` | `A` | `29.350` | `2.000` | `Speech` | `0.000`

From left to right, the columns in this file contain:

- The channel number, usually `1`.
- A fixed field, `A`.
- The time in seconds from the beginning of the audio to the start of the segment.
- The duration in seconds of the segment.
- The segment classification–either `Silence`, `Music/Noise`, or `Speech`.

## Clipping Detection Mode

The following is an example of results produced by the clipping detection mode.

    <audiopreproc>
    	<clipping>
    		<assessment>none</assessment>
    		<percent_frames>0</percent_frames>
    	</clipping>
    </audiopreproc>

IDOL Speech Server returns both a qualitative assessment of the clipping and the percentage of affected frames.

## SNR Calculation Mode

The following is an example of results produced by the SNR calculation mode.

`0.01` | `2.5` | `22`
`2.84` | `5.33` | `25`
`6.62` | `7.12` | `25`
`7.12` | `9.05` | `24`
`9.05` | `9.71` | `24`
`9.71` | `12.2` | `23`
`13.43` | `14.15` | `24`
`14.15` | `14.82` | `28`
`14.82` | `17.11` | `22`
`17.11` | `19.6` | `25`
`20.17` | `20.67` | `17`
`20.67` | `21.41` | `29`
`21.41` | `23.9` | `21`

From left to right, the columns in this file contain:

- The time in seconds from the beginning of the audio to the start of a section of speech.
- The time in seconds from the beginning of the audio to the end of the section of speech.
- The SNR for the speech segment.

## DTMF Mode

The following is an example of results produced by the DTMF mode.

`1` | `A` | `0.000` | `0.020` | `none` | `0.000`
`1` | `A` | `0.020` | `0.300` | `<DTMF-0>` | `53.942`
`1` | `A` | `0.320` | `1.040` | `none` | `0.000`
`1` | `A` | `1.360` | `0.300` | `<DTMF-1>` | `54.591`
`1` | `A` | `1.660` | `1.040` | `none` | `0.000`
`1` | `A` | `2.700` | `0.320` | `<DTMF-2>` | `52.078`
`1` | `A` | `3.020` | `1.030` | `none` | `0.000`
`1` | `A` | `4.050` | `0.320` | `<DTMF-3>` | `52.085`
`1` | `A` | `4.370` | `1.040` | `none` | `0.000`
`1` | `A` | `5.410` | `0.310` | `<DTMF-4>` | `53.31`

From left to right, the columns in this file contain:

- The channel number, usually `1`.
- A fixed field, `A`.
- The time in seconds from the beginning of the audio to the boundary between the dial tone and other audio.
- The duration in seconds of the dial tone or the period of audio between dial tones.
- The segment classification–if IDOL Speech Server detects a dial tone, it identifies the tone.
- The score for the tone identification.

© 2013-2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm