Open topic with navigation

# [postproc] Module Configuration

The `postproc` module filters and modifies results produced by audio processing tasks such as speech-to-text, language identification, and so on.

## Input and Output

The `postproc` module has two modes of operation, which can also be combined to perform both processes in a single operation.

Mode | Input | Output | Description
--- | --- | --- | ---
`B` | `w` | `w` | Accepts a word data stream, and replaces all barred words either with a fixed term (such as `<BLEEP>`), or a term specific to an individual word. The barred word list is provided as a text file containing one word or a pair of words (the barred word, and the replacement term for that word) on each line.
`R` | `w` | `w` | Accepts a data stream, and recombines any word fragments to form complete words. Writes the resulting word sequence to an output word stream.

Examples:

    w2 ← postproc (B,w1)

    w2 ← postproc (R,w1)

    w2 ← postproc (BR,w1)

## Parameters

Note: In `B` mode, you must set at least one of the `BarredList` and `BarredTerm` parameters.

BarredList
BarredTerm
RcmpAllowSuffix
RcmpValidList

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm