Open topic with navigation

# BinaryDataPort

The `BinaryDataPort` parameter sets the port number to receive live streaming audio. This port must not be used by any other program.

Type: | Integer
Default: | 16000
Allowed Range: | Minimum: 0 Maximum: 65536
Recommended Range: | Minimum: 1025 Maximum: 65536
Required: | Yes
Configuration Section: | Server
Example: | `Port=16000`
See also: |

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm