Open topic with navigation

# MaxSilThresh

The threshold between what the module identifies as silence and non-silence.

Type: | Integer
Default: | 50
Recommended Range: | Minimum: 20 Maximum: 100
Required: | No
Configuration Section: | audiopreproc and splitspeech modules
Example: | `MaxSilThresh=60`
See Also: | SilThresh (action parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm