Open topic with navigation

# USMFile

The Universal Speech Model to use.

You must set the value of this parameter to match the value that you used during optimization.

Type: | String
Default: | The default value is derived from the base Speaker ID pack.
Required: | No
Configuration Section: | sidpackager module
Example: | `USMFile=baseModel.usm`
See also: | USM (action parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm