Open topic with navigation

# SpeechThresh

The threshold between speech and non-speech (music or noise).

Action: | AddTask, CheckResources
Task: | SpeechSilClassification
Type: | Integer
Default: | -25
Range: | -50–10
Example: | `SpeechThresh=0`
See Also: | SpeechThreshOffset (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm