Open topic with navigation

# SpeechThreshOffset

The threshold between speech and non-speech (music or noise).

Type: | Integer
Default: | -25
Recommended Range: | Minimum: -50 Maximum: 10
Required: | No
Configuration Section: | audiopreproc and splitspeech modules
Example: | `SpeechThreshOffset=-15`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm