Open topic with navigation

# [segment] Module Configuration

The `segment` module attempts to identify approximate speaker change points in the audio.

To identify speakers in the audio, use the `speakerid` module.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `nf` | `w` | Performs speaker segmentation and broad classification.

Example:

    w <- segment (_, nf)

## Parameters

IANFile | SegMin
OutFile* | Sensitivity
OutFileLabel | WavFile
SegMax |

*You must set the value of this configuration parameter by setting the corresponding action parameter.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm