Open topic with navigation

# [sidoptimizer] Module Configuration

The `sidoptimizer` module generates statistics that are used to optimize the individual speaker match thresholds, leading to an optimized system.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `a` | `f` | Accepts audio data, and produces feature frames.

Example:

    f <- sidoptimizer(_, a)

## Parameters

BaseAstFile* | SpeakerName*
CompSelect * | SpkIDBasePack
Diag | SpkListFile*
DiagFile | SpkListPath
DiagFileLabel | SpkSegmentCoef
DiscardShortSegs | SpoAppend
MinNonSpeech | SpoFile*
MinSpeech | TempDir
SampleFrequency* | USMEnabled *
SigFile* | USMFile *

*You must set the value of these configuration parameters by setting the corresponding action parameters.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm