Open topic with navigation

# Gb_MinDuration

The `GB_MinDuration` parameter specifies the minimum time duration for a sequence of tones, in breaking glass detection.

Type: | Integer
Default: | 50
Recommended Range: | 25–100
Required: | No
Configuration Section: | audiosec module
Example: | `Gb_MinDuration=50`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm