Open topic with navigation

# Sc_MinScreamLen

The `Sc_MinScreamLen` parameter specifies the minimum length of a scream in seconds.

Type: | Decimal
Default: | 0.4
Recommended Range: | 0.2–1.0
Required: | No
Configuration Section: | audiosec module
Example: | `Sc_MinScreamLen=0.4`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm