Open topic with navigation

# [audiosec] Module Configuration

The `audiosec` module detects security-related audio signals including alarms, screams, gunshots, and breaking glass.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `a, nf` | `w` | The `audiosec` module requires both raw audio data and normalized frontend feature frames.

Example:

    w <- audiosec(_, a,nf)

## Parameters

Al_AllowUnkAlarm | Gb_EdgeMaxDist | Model
Al_GenThreshold | Gb_EdgeTrigger | SampleFrequency
Al_MaxPeriod | Gb_MinDuration | Sc_MinScreamLen
Al_TemplateListFile | Gb_MinOutScore | Sc_MinScreamPitch
Al_TemplatePath | Gb_MinStreaks | Sc_MinScreamSegScore
Al_TmThreshold | Gs_EdgeTrigger |

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm