Open topic with navigation

# SpkIdTrainWav

The `SpkIdTrainWav` task takes a single audio file containing speech data from the speaker to be trained, and creates a new speaker template file.

Note: To process streamed audio, use the SpkIdTrainStream task.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task name. Set to `SpkIdTrainWav`. | Yes
DiagFile | The file to write the diagnostic information to. |
DiagLevel | The level of detail to include in the diagnostic information. |
File | The audio file that contains sample speech from one person. | Yes
LabExt | The file extension to use for label files. | Yes, if your files have an extension other than the default (`.lab`)
LabFile | A single label file to use. |
LabPath | The path to the label files. | Yes, if you have enabled labeling and are specifying a list of multiple files to use
LabType | The type of labels to use. |
Out | The name of the speaker template file to create. You must include the audio template file extension ( `.atf` ) . | Yes
Sfreq | The sample frequency of the audio file to process. |
SugdInputChannels | The channel layout of the input media file. |
SugdInputFrequency | The sampling rate of the input media file. |
UBMFile | The Universal Background Model to use. |

## Example

`http://localhost:15000/action=AddTask&Type=SpkIdTrainWav&File=C:/Data/BrownSpeech.wav&Out=Brown.atf`

This action uses port `15000` to instruct IDOL Speech Server, which is located on the local machine, to create the `Brown.atf` template file by using the `BrownSpeech.wav` file.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm