Open topic with navigation

# ModeValue

The meaning of this parameter depends on the value of the Mode parameter:

- If the `Mode` parameter is set to `fixed`, `ModeValue` specifies the beam width to use. The beam width affects how IDOL Speech Server searches for recognized word sequences. You can set a value between 1.0 and 4.0. A higher beam width can produce a more accurate transcription but processing might be slower.
- If the `Mode` parameter is set to `relative`, `ModeValue` specifies a factor that represents the data processing rate compared to real time. You can set a value between 0.25 and 4.0. A value of `0.25` processes data four times as fast as real time, while `4.0` processes data four times slower than real time. The higher the value, the longer processing takes.

Type: | Number
Default: |
Required: | Yes
Configuration Section: | TaskName
Example: | `ModeValue=3.0`
See Also: | Mode

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm