Open topic with navigation

# NTLMPassword

The NT password to use to retrieve video from the Milestone surveillance system. To use NT credentials you must set SOAPAuthentication to `true`.

Note: HPE recommends encrypting user names and passwords before entering them in configuration files. For information about how to do this, refer to the Media Server Administration Guide.

Type: | String (can be encrypted)
Default: |
Required: | No
Configuration Section: | TaskName
Example: | `NTLMPassword=yL7f9q8u0lg5f`
See Also: | NTLMUserName

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm