Open topic with navigation

# InverseOption

Specifies whether Media Server considers inverse formats when detecting and reading number plates.

Inverse formats usually represent a small proportion of number plates, where the expected color of the number plate differs from the standard format. For example, a standard UK number plate has black characters on a white background. A small proportion of UK number plates have white characters on a black background, and these are defined in the formats file as inverse formats.

Set this parameter to one of the following options:

- `PrioritiseNormal` - Media Server prioritizes normal formats, and only considers inverse formats if a number plate candidate is detected in a region with colors that match an inverse format. This option results in faster processing than `BothFully`.
- `BothFully` - Media Server considers both normal and inverse formats.
- `NormalOnly` - Media Server considers only normal formats.
- `InverseOnly` - Media Server considers only inverse formats.

Type: | String
Default: | PrioritiseNormal
Required: | No
Configuration Section: | TaskName
Example: | `InverseOption=NormalOnly`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm