Open topic with navigation

# OutputURL

The URL to stream video to.

When streaming encoded video, you must also set the Format parameter.

Type: | String
Default: |
Required: | Required to encode video to an IP stream
Configuration Section: | TaskName
Example: | `OutputURL=udp://239.255.1.123:4321`
See Also: | Format

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm