Open topic with navigation

# ThreadCount

The maximum number of threads to use to detect and read number plates. For example, if you set `ThreadCount=3`, Media Server can process up to three frames simultaneously.

Type: | Integer
Default: | 2
Required: | No
Configuration Section: | TaskName
Example: | `ThreadCount=4`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm