Open topic with navigation

# Audio Fingerprint Identification

The following schema describes how to define an audio fingerprint (AFP) identification task.

    [AFPMatchWav]
    0 = a ← wav(MONO, input)
    1 = fp ← afpfeature(_, a)
    2 = tr ← afp(_, fp)
    3 = output ← afpout(_, tr)

`0` | The `wav` module processes the mono audio.
`1` | The `afpfeature` module converts audio data into audio fingerprint features.
`2` | The `afp` module matches features against a database of known tracks.
`3` | The `afpout` module writes the identification results to file.

© 2013-2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm